How-to guide template
From any2.video/resources/how-to-write-step-by-step-instructions. One task, numbered steps, a finish line.
	Title
	The task as a verb phrase: 'Restore a file from last night's backup'.

	Applies to
	Product, version and the date the steps were last checked.

	Before you start
	Accounts, permissions, files and anything that must already be set up.

	Done when
	The result the reader will see, and how they can check it.


Steps
	#
	Do this
	You should see
	Image or clip

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	


If it goes wrong
	Symptom
	Cause and fix

	
	

	
	

	
	




Worked example: Install Proxmox VE 9.2 on a blank machine
	Title
	Install Proxmox VE 9.2 on a blank machine

	Applies to
	Proxmox VE 9.2; steps checked against a real run on 2026-09-01.

	Before you start
	A blank 64-bit machine (the installer takes the whole disk), a USB stick, the ISO and its published checksum.

	Done when
	The web interface opens on port 8006 at the address you set, and you can log in as root.


	#
	Do this
	You should see
	Image or clip

	1
	Download the ISO and check it against the published checksum before writing it.
	The checksum matches the published one
	01:23

	2
	Boot the installer and accept the licence.
	The target disk screen
	

	3
	Choose the target disk; pick ext4 on a single disk.
	Disk and filesystem selected
	02:46

	4
	Set country, timezone, keyboard, root password and email.
	The network screen
	

	5
	Fill in hostname, CIDR IP, gateway and DNS, one field at a time.
	A summary with your network values
	04:59

	6
	Install, remove the USB stick and reboot.
	The console prints the URL to open
	06:04

	7
	Open the URL on port 8006 and log in as root.
	The Proxmox VE web interface
	06:35


If it goes wrong
Expecting to keep the existing operating system on the disk. The installer takes the entire disk and cannot dual boot or resize a partition, so back up anything already on that disk first or use a second disk.
Install completes but the web interface is unreachable. The cause is almost always the network screen: an IP outside the LAN's range, a missing gateway or a wrong CIDR suffix. That is why the video goes through that screen one field at a time.




